**Distributor Support: EnduraRamp™ Description**

**EnduraRamp™ Bio**

The EnduraRamp™ slows down traffic at your worksite, school or wherever traffic calming is required. This speed bump is durable and easy to install.

**Features & Benefits**

* Thick plastic moulded coloured skin which provides long-lasting hi-vis colours
* Lightweight and durable solution for easy installation
* Dog bone locators help to align the ramps during installation
* Manage the speed of traffic effectively across site and pedestrian areas
* Protect site staff and pedestrians against traffic and vehicles
* Create highly-visible traffic management solutions with in built reflective
* Support road traffic, vehicles and cargo up to 44 tonnes
* Designed to be installed on good condition concrete or asphalt surfaces that are at least 100mm deep
* Run cabling and piping of up to 22mm diameter within the ramp’s recess
* 100% recyclable
* A closed loop recycling product: made of recycled PVC
* Enquire about minimum order quantities for customisations

**EnduraRamp™ – Technical Specification**

|  |  |  |
| --- | --- | --- |
| **INNER** | **50mm** | **75mm** |
| Product SKU No. | 779 | 2483 |
| Product No. | 0376 | 0321 |
| Length | 500mm | 500mm |
| Width | 420mm | 420mm |
| Height | 50mm | 75mm |
| Weight | 9kg | 12kg |
| Qty/Pallet | 100 | 100 |
| Colour | Yellow & Black (White on request) | Yellow & Black (White on request) |

|  |  |  |
| --- | --- | --- |
| **END** | **50mm** | **75mm** |
| Product SKU No. | 636 | 664 |
| Product No. | 0377 | 0323 |
| Length | 210mm | 210mm |
| Width | 420mm | 420mm |
| Height | 50mm | 75mm |
| Weight end | 3.5kg | 4.5kg |
| No. Per pallet | 120 | 100 |
| Slows traffic to | 10mph | 5mph |
| Colour | Yellow & Black (White on request) | Yellow & Black (White on request) |

**Recommended SEO for EnduraRamp**

H1 Title: EnduraRamp™

H2 Title: EnduraRamp™ Speed Bumps

Meta Tile: EnduraRamp™ | Plastic Speed Bumps | Oxford Plastics

Meta Description: EnduraRamp™ Plastic Speed Bumps are ideal for schools and areas which call for low traffic speeds, available in 2 colours for high-visibility contrast.