**Distributor Support: EnduraSign QuickFit Frame® & EnduraSign Ballast Description**

**EnduraSign QuickFit Frame® Bio**

The EnduraSign QuickFit® Frame is a plastic sign frame that is compatible with 300mm hole centre

sign faces. The modular design means the correct signage can be quickly assembled on site. Space and weight limitations are improved in works vehicles compared to using 1 piece Chapter 8 signs.

**Features & Benefits**

* Ultra-durable sign frame is resistant to cracking
* Plastic sign frame fitted with 4 antiluce droplocks, compatible with 300mm spaced quickfit faces
* Compact design to take up less space in works vehicles
* Lightweight 3.3kg design reduces weight in works vehicles
* Interchangeable sign faces can be installed on-site
* Highly resistant to wind
* Category C (19 mph) winds without ballast
* Category B (39 mph) winds with a 9kg weight (for 1050 rectangle use 13kg)
* Compatible with EnduraSign Ballast 9kg weight
* Clearly label equipment and prevent theft with a corporate nameplate and custom RAL colour frame. Enquire about minimum order quantities for customisations
* Create clear signage and information in all weather

**EnduraSign Ballast Bio**

The EnduraSign Ballast can be used on all metal and plastic temporary signs to ensure that temporary works stay clearly signposted and street works compliant. This ballast weight replaces sandbags, it is stackable, quick to deploy and is significantly longer-lasting.

**Features & Benefits**

* Fits EnduraSign QuickFit Frame®
* Fits Q-Sign
* Fits metal signs
* Replaces sandbags
* Leaves no debris
* Hi-vis edges
* 100% recyclable
* Contact Oxford Plastics about returning end of life products for recycling or reuse
* Enquire about minimum order quantities for customisations

**EnduraSign QuickFit Frame® & EnduraSign Ballast – Technical Specification**

|  |  |  |
| --- | --- | --- |
|  | EnduraSign QuickFit Frame® | EnduraSign Ballast |
| Product SKU No. | 5480 | 4805 |
| Product No. | 0424 | 0426 |
| Height | 870mm | 90mm |
| Width | 35mm | 556mm |
| Length | 800mm | 407mm |
| Weight | 3.3kg | 10kg |
| Qty/Pallet | 50 | 60 |
| Colour | Black (Custom RAL Colours, MOQ) | Black with Yellow HiVis edges |

**Recommended SEO for EnduraSign QuickFit Frame**®

H1 Title: EnduraSign QuickFit Frame®

H2 Title: Chapter 8 Streetworks Temporary Road Sign

Meta Tile: EnduraSign QuickFit Frame® | Temporary Road Signs - Oxford Plastics

Meta Description: Discover our long-life, temporary and patented plastic traffic sign. Compatible with 300mm hole centred quick-fit Chapter 8 sign faces.

**Recommended SEO for EnduraSign Ballast**

H1 Title: EnduraSign Ballast

H2 Title: Sign weight for plastic & metal signs

Meta Tile: EnduraSign Ballast | Plastic & Metal Signs | Oxford Plastics

Meta Description: Use the EnduraSign ballast on all temporary signs; the Q-Sign, metal signs and more!, The EnduraSign Ballast is the only sign weight of its kind