**Distributor Support: Avalon**® **Barrier Description**

**Avalon**® **Chapter 8 Barrier Bio**

The Avalon® is our most versatile and popular safety barrier. It is compliant with street works regulations and suitable for a wide range of indoor and outdoor pedestrian applications. Common uses include construction, excavation, street works, events and utilities sites.

Oxford Plastics’ StrongWall Ballast is a heavy duty and firm solution to barrier stability. It also complies with Wind Loading Class B regulations.

Ballast Trays are an anchor system to give extra stability in strong winds. Fill with spoil from site or the OxBlock to create a semi-permanent work site perimeter.

**Features & Benefits**

* The original Chapter 8 Safety Barrier
* Available in 2m, 1m & 0.5m sizes
* Can be easily transported and stored
* Adaptable to the work site’s requirements with 2 feet options: ClearPath Extra which is 100% antitrip or standard
* Compliant with the Red Book, Chapter 8 Street Works,BS 7818 and BS 8442:2006
* Suitable for indoors and outdoors
* Patented tamper-proof Avalon® Fishtail (hook & pin) linking system to protect site staff and pedestrians against risk factors
* Ballast option up to category A wind loading: StrongWall base
* Single piece, light, blow moulded pedestrian barrier made of high-density polythene (HDPE)
* Use on uneven ground
* Fix signage, adverts & contractor information
* Designed and manufactured in the UK
* 100% recyclable
* Contact Oxford Plastics about returning end of life products for recycling or reuse
* Enquire about minimum order quantities for customisations

**Avalon**® **Chapter 8 Barrier – Technical Specification**

|  |  |  |  |
| --- | --- | --- | --- |
|  | Avalon® 2m | Avalon® 1m | Avalon® 0.5m |
| Product SKU No. | 3802 | 4186 | 4738 |
| Product No. | 0635 | 0634 | 0646 |
| Height | 1000mm | 1000mm | 1000mm |
| Width | 40mm | 40mm | 40mm |
| Length | 2005mm | 1000mm | 655mm |
| Weight | 11kg | 8.5kg | 1.8kg |
| Qty/Pallet | 50 | 50 | 100 |
| Colour | Orange, other colours available | Orange, other colours available | Orange, other colours available |

|  |  |
| --- | --- |
|  | StrongWall Ballast |
| Product SKU No. | 4187 |
| Product Number | 0197 |
| Height | 300mm |
| Width | 520mm |
| Length | 1000mm |
| Weight | 18kg |
| Qty/Pallet | 18 |
| Colour | Black |

**Recommended SEO for Avalon**® **Barrier**

H1 Title: Avalon® Chapter 8 Barrier

H2 Title: Plastic Road & Safety Barriers

Meta Tile: Avalon® Barrier & Plastic Barriers | Oxford Plastics

Meta Description: Oxford Plastics offer an extensive range of plastic safety barriers. Browse our Chapter 8 Avalon® safety barriers, perfect for construction sites.

**Videos**

Avalon® Barrier - <https://www.youtube.com/watch?v=qDCauMHNHy0>

Avalon® Barrier, Right to Repair - <https://www.youtube.com/watch?v=-qxzT3PdN0Q>

Chapter 8 Street Works Explained - <https://www.youtube.com/watch?v=8agZ0LKfZGU>