**Distributor Support: EnduraGrid™ Description**

**EnduraGrid™ Bio**

EnduraGrid™ is an interlocking porous paving system designed to reinforce the ground. Perfect for carparks, driveways, paths, patios and muddy areas.

**Features & Benefits**

* Create permanent ground protection grids
* Lightweight and durable for easy transport and installation by 1 person
* Prevents gravel migration and soil erosion
* Interlock the paving system to reinforce the ground
* Parking marker spots slot into the grid to demarcate car park spaces
* Anti-Slip surface reinforcement with natural drainage
* Expands and contracts with the weather
* Allows grass to grow through and disguise the grids
* Provides improved water dispersion
* No expensive equipment needed
* Suitable for 44 tonnes vehicles
* Can be easily cut to size
* Curved lattice structure creates a flat surface: the grid allows for expanding and contracting in hot weather to prevent the surface from rounding up
* Quick and easy installation: 3900 ft² per hour (depending upon ground preparation)
* Eco-friendly car park solution with natural drainage
* 100% recyclable
* Contact Oxford Plastics about returning end of life products for recycling or reuse

**EnduraGrid™ – Technical Specification**

|  |  |  |
| --- | --- | --- |
| **EnduraGrid™** | Grid | Marker |
| Product SKU No. | 3463 | 3600 |
| Product No. | 0681 | 0684 |
| Width | 500mm | 69mm |
| Length | 500mm | 69mm |
| Height | 65mm | 68mm |
| Weight | 2kg | N/A |
| Quantity/Pallet | 120 | 100 |
| Colour | Black | White/Yellow |

**Recommended SEO for EnduraGrid™**

H1 Title: EnduraGrid™

H2 Title: Plastic Pavers & Gravel Grids

Meta Tile: Plastic Pavers | Plastic Gravel Grid | EnduraGrid™ | Oxford Plastics

Meta Description: EnduraGrid™ Plastic paving grids are permanent ground protection grids for carparks. Browse our EnduraGrid™ plastic pavers now to learn more.