**Distributor Support: SafeGate & SafeBase Description**

**SafeGate & SafeBase Bio**

The SafeGate barrier is designed for use around temporary excavations and commonly used in the communications industry. The SafeGate can be configured in a square or in a line with the SafeBase.

**Features & Benefits**

* Portable 1-person gate barrier
* Compliant with Chapter 8 Street Works
* Guarding manholes & temporary excavations
* Portable - fits in the back of a van, lightweight for 1 person jobs
* Use 4 x SafeBase on SafeGate to pass wind loading category A
* Set of 3 or 4 hi-vis, hinged gates
* Lightweight: each gate weighs just 2kg, keeps overall vehicle weight low, and allows for easy installation
* Modular design for various configurations
* Keep sites protected in high wind conditions by using the SafeBase
* Hinged clips for quick and easy assembly
* Integral locking clamp for stability when barriers are deployed in a straight line
* Made from high-density polyethylene (HDPE)
* Designed and manufactured in the UK
* 100% recyclable
* Contact Oxford Plastics about returning end of life products for recycling or reuse
* Enquire about minimum order quantities for customisations

**SafeGate & SafeBase** **– Technical Specification**

|  |  |  |  |
| --- | --- | --- | --- |
| SafeGate | 3 Gate | 4 Gate | SafeBase |
| Product SKU No. | 5069 | 3609 | 4627 |
| Product No. | 09737 | 09738 | 0204 |
| Length | 2250mm | 3000mm | 340mm |
| Height | 1000mm | 1000mm | 80mm |
| Width | 60mm | 80mm | 340mm |
| Weight | 6kg | 8kg | 2.6kg |
| Qty/Pallet | 25 | 20 | 150 |
| Colour | Red, Yellow also available | Red, Yellow also available | Black |

**Recommended SEO for SafeGate & SafeBase**

H1 Title: SafeGate

H2 Title: SafeGate Barrier Manhole Guard

Meta Tile: SafeGate Barrier & Plastic Gate Barrier | Oxford Plastics

Meta Description: Our SafeGate® barrier is light and portable, making it ideal for manhole repairs and the telecoms industry. Browse our SafeGate barriers and plastic gate barriers.