**Distributor Support: NEW LowPro® 15/05 Road Plate Description**

**NEW LowPro® 15/05 Road Plate Bio**

Our NEW LowPro® 15/05 Road Plates allow vehicles, pedestrians and wheelchair users to safely travel across trenches up to 700mm wide. Suitable for vehicles up to 44 tonnes, these composite, lightweight road plates are excellent alternatives to steel road plates.

**Features & Benefits**

* Compatible with LowPro 15/05 MKI
* Suitable for 44T vehicles over a 700mm trench
* Complies with HAUC’s 2018/01 Advice Note
* Can be easily transported and stored by 2 people using Easilift handles or handhold points
* Drop-pins prevent lateral movement
* Moulded anti-slip surface
* Flat top for stable stacking
* Hi Vis yellow encourages traffic calming
* Patented LowPro edges reduce noise pollution
* Maintain quality and performance with spare parts, if necessary
* Reduce CO2 emissions with lighter transport compared to steel plates
* Designed & manufactured in the UK
* Contact Oxford Plastics about returning end of life products for recycling or reuse
* Enquire about minimum order quantities for customisations

**LowPro® 15/05 Road Plate** **– Technical Specification**

|  |  |  |
| --- | --- | --- |
| LowPro**®** 15/05 | 15/05 Inner | 15/05 End |
| Product SKU No. | 5792 | 5790 |
| Product No. | 0900 | 0903 |
| Length | 1500mm | 1500mm |
| Width | 500mm | 500mm |
| Height | 75mm | 75mm |
| Weight | 40kg | 10kg |
| Qty/Pallet | 20 | 20 |
| Colour | Yellow & Blue | Blue |

**Recommended SEO for LowPro® 15/05 Road Plate**

H1 Title: NEW LowPro® 15/05 Road Plate

H2 Title: NEW LowPro® 15/05 Plastic Road Plates

Meta Tile: Plastic Road Plates | LowPro**®** 15/05 | Oxford Plastics

Meta Description: The NEW LowPro® 15/05 is made of modular plastic road plates, suitable for 44t vehicles, and for carriageways over a 700mm trench. Browse our plastic road plates.

**Videos**

LowPro Road Plates - <https://www.youtube.com/watch?v=JeX-mpzDAhw&t>

LowPro Trench Cover & Road Plate Range - <https://www.youtube.com/watch?v=Q14Er_Z9UCQ>