**Distributor Support: Bypass Ramp Description**

**Bypass Ramp Bio**

The Bypass Ramp is an access ramp for when pipeline is diverted above ground. Allowing vehicles up to 97,000 to traverse pipes up to 4.5” dia. Replacing single-use cold patch ramps.

**Features & Benefits**

* Eliminates asphalt cold patch ramps
* Gives ramped access to homes
* Reusable, repairable & recyclable
* Adaptable to curb heights
* Load rated up to 97,000 vehicles
* Accepts pipes up to 4.5” dia., which must be load-bearing
* Accepts non-load-bearing pipes up to 3.5” dia.
* Must be anchored to the ground
* Non-slip top surface.
* One-person installation, quick to deploy in sections that link easily
* Contact Oxford Plastics about returning end-of-life products for recycling or reuse
* Enquire about minimum order quantities for customisations

**Bypass Ramp – Technical Specification**

|  |  |
| --- | --- |
|  | Bypass Ramp |
| Product SKU No. | 5949 |
| Product No. | 0920 |
| Length | 50” |
| Height | 5” |
| Width | 18” |
| Weight | 21lbs |
| Qty/Pallet | 25 |
| Colour | Yellow |

**Recommended SEO for Bypass Ramp**

H1 Title: Bypass Ramp

H2 Title: Bypass Access Ramp

Meta Tile: Bypass Ramp for Access| Oxford Plastics

Meta Description: The Bypass Ramp is an access ramp for when pipeline is diverted above ground. Allowing vehicles up to 97,000 to traverse pipes up to 4.5” dia. Replacing single-use cold patch ramps.