**Distributor Support: EnduraFence™ Description**

**EnduraFence™ Bio**

Heavy duty plastic fence that is 2m tall and anti-climb, making it suitable for construction, deep excavation and street works sites. It is ideal for when metal fencing cannot be used.

**Features & Benefits**

* 2m non-conductive fencing
* Outlasts metal fencing
* Non-conductive, for use in Rail & around live electricity
* Chapter 8 compliant
* 2m anti-climb Enhanced barrier
* Durable and lightweight
* Compact stacking for easy transportation and storage
* 1-person assembly
* Links to steel mesh fencing
* Designed and manufactured in the UK
* 100% recyclable
* Contact Oxford Plastics about returning end of life products for recycling or reuse
* Enquire about minimum order quantities for customisations

**EnduraFence™ – Technical Specification**

|  |  |
| --- | --- |
|  | **EnduraFence™** |
| Product SKU No. | 3001 |
| Product No. | 0668 |
| Length | 1900mm |
| Height | 1900mm |
| Width | 40mm |
| Weight | 10Kg |
| Qty/Pallet | 32 |
| Colour | Orange (other colours on request) |

**Recommended SEO for EnduraFence™**

H1 Title: EnduraFence™

H2 Title: Heavy Duty Plastic Barrier

Meta Tile: Plastic Barrier Fence| EnduraFence™ | Oxford Plastics

Meta Description: Oxford Plastics offer durable and heavy duty plastic barriers. EnduraFence™ plastic barriers are customisable.

**Videos**

Chapter 8 Street Works Explained - https://www.youtube.com/watch?v=8agZ0LKfZGU