**Distributor Support: Oxford LowPro 11/11 Pedestrian Mat Description**

**Oxford LowPro 11/11**

Pedestrian board with patented LowPro Edge technology, suitable for the distributed load of a 3528lb vehicle over a 28” trench.

**Features & Benefits**

* 1 person-lift pedestrian mat
* Extremely compact and flat making it easy to transport & store
* Safely cover holes and trenches up to 28”
* Hi-vis and anti-trip trench cover provides safe passageway for pedestrians and vehicles up to 3,528lb
* Oxford LowPro edges grip the asphalt – pinning not required in most applications
* Moulded anti-slip surface
* Not for use in roadway
* Trench covers must be installed centrally over the trench
* Shock resistant
* Eliminate need for cold patch with the patented LowPro Edge, which provides smooth transition
* Reduce CO2 emissions with lighter transport compared to steel plates
* Designed & manufactured in the UK
* Enquire about minimum order quantities for customizations

**Oxford LowPro 11/11 Pedestrian Mat** **– Technical Specification**

|  |  |
| --- | --- |
|  | LowPro 11/11 |
| Product SKU No. | 3147 |
| Product No. | 0815 |
| Length | 44” |
| Width | 44” |
| Height | 1” |
| Weight | 53lb |
| Qty/Pallet | 30 |
| Color | Yellow & Black |

**Recommended SEO for Oxford LowPro 11/11 Pedestrian Mat**

H1 Title: Oxford LowPro® 11/11 Trench Cover

H2 Title: Composite Pedestrian Board

Meta Tile: Oxford LowPro 11/11 | Pedestrian Mat | Oxford Plastics

Meta Description: The Oxford LowPro 11/11 pedestrian board is part of the LowPro Trench Cover range and is suitable for the distributed load of 3,528lb over a 28” trench.

**Videos**

LowPro Trench Covers - <https://www.youtube.com/watch?v=rBSKmoWFVKc>

LowPro Trench Cover & Road Plate Range - <https://www.youtube.com/watch?v=Q14Er_Z9UCQ>